#version 420
#extension GL_ARB_texture_gather : enable
#extension GL_ARB_separate_shader_objects : enable
#ifdef VULKAN
#define ATTR_LAYOUT(__vkSet, __location) layout(set = __vkSet, location = __location)
#define UNIFORM_BUFFER_LAYOUT(__glLocation, __vkSet, __vkLocation) layout(set = __vkSet, binding = __vkLocation, std140)
#define TEXTURE_LAYOUT(__glLocation, __vkSet, __vkLocation) layout(set = __vkSet, binding = __vkLocation)
#define SET_POSITION(_v) gl_Position = _v; gl_Position.z = (gl_Position.z + gl_Position.w) / 2.0
#define GET_FRAGCOORD() vec4(gl_FragCoord.xy*uf_fragCoordScale.xy,gl_FragCoord.zw)
#define gl_VertexID gl_VertexIndex
#define gl_InstanceID gl_InstanceIndex
#else
#define ATTR_LAYOUT(__vkSet, __location) layout(location = __location)
#define UNIFORM_BUFFER_LAYOUT(__glLocation, __vkSet, __vkLocation) layout(binding = __glLocation, std140) 
#define TEXTURE_LAYOUT(__glLocation, __vkSet, __vkLocation) layout(binding = __glLocation)
#define SET_POSITION(_v) gl_Position = _v
#define GET_FRAGCOORD() vec4(gl_FragCoord.xy*uf_fragCoordScale,gl_FragCoord.zw)
#endif
/* This shaders was auto-converted from OpenGL to Cemu.
Conversion output:
*/

#define gsswDefault $gsswDefault
const vec3 Color = vec3($gsswR,$gsswG,$gsswB);
const float Factor = $gsswL_f;

// Guardian Stalker + Scout + Guardian weapons

// shader 91b6e09da2ff63cc
#ifdef VULKAN
layout(set = 1, binding = 6) uniform ufBlock
{
uniform ivec4 uf_remappedPS[3];
uniform vec4 uf_fragCoordScale;
};
#else
uniform ivec4 uf_remappedPS[3];
uniform vec2 uf_fragCoordScale;
#endif
// uf_fragCoordScale was moved to the ufBlock
TEXTURE_LAYOUT(1, 1, 0) uniform sampler2D textureUnitPS1;
TEXTURE_LAYOUT(2, 1, 1) uniform sampler2D textureUnitPS2;
TEXTURE_LAYOUT(3, 1, 2) uniform sampler2D textureUnitPS3;
TEXTURE_LAYOUT(4, 1, 3) uniform sampler2D textureUnitPS4;
TEXTURE_LAYOUT(5, 1, 4) uniform sampler2D textureUnitPS5;
TEXTURE_LAYOUT(6, 1, 5) uniform sampler2D textureUnitPS6;
layout(location = 0) in vec4 passParameterSem0;
layout(location = 1) in vec4 passParameterSem1;
layout(location = 2) in vec4 passParameterSem7;
layout(location = 3) in vec4 passParameterSem3;
layout(location = 4) in vec4 passParameterSem4;
layout(location = 5) in vec4 passParameterSem6;
layout(location = 0) out vec4 passPixelColor0;
layout(location = 1) out vec4 passPixelColor1;
layout(location = 3) out vec4 passPixelColor3;
layout(location = 5) out vec4 passPixelColor5;
int clampFI32(int v)
{
if( v == 0x7FFFFFFF )
	return floatBitsToInt(1.0);
else if( v == 0xFFFFFFFF )
	return floatBitsToInt(0.0);
return floatBitsToInt(clamp(intBitsToFloat(v), 0.0, 1.0));
}
float mul_nonIEEE(float a, float b){ if( a == 0.0 || b == 0.0 ) return 0.0; return a*b; }
void main()
{
vec4 R0f = vec4(0.0);
vec4 R1f = vec4(0.0);
vec4 R2f = vec4(0.0);
vec4 R3f = vec4(0.0);
vec4 R4f = vec4(0.0);
vec4 R5f = vec4(0.0);
vec4 R6f = vec4(0.0);
vec4 R7f = vec4(0.0);
vec4 R122f = vec4(0.0);
vec4 R123f = vec4(0.0);
vec4 R124f = vec4(0.0);
vec4 R125f = vec4(0.0);
vec4 R126f = vec4(0.0);
vec4 R127f = vec4(0.0);
float backupReg0f, backupReg1f, backupReg2f, backupReg3f, backupReg4f;
vec4 PV0f = vec4(0.0), PV1f = vec4(0.0);
float PS0f = 0.0, PS1f = 0.0;
vec4 tempf = vec4(0.0);
float tempResultf;
int tempResulti;
ivec4 ARi = ivec4(0);
bool predResult = true;
vec3 cubeMapSTM;
int cubeMapFaceId;
R0f = passParameterSem0;
R1f = passParameterSem1;
R2f = passParameterSem7;
R3f = passParameterSem3;
R4f = passParameterSem4;
R5f = passParameterSem6;
R5f.xy = (texture(textureUnitPS3, R0f.xy).xy);
R1f.w = (texture(textureUnitPS2, R0f.xy).x);
R7f.xyz = (texture(textureUnitPS4, R0f.xy).xyz);
R6f.xyz = (texture(textureUnitPS5, R0f.zw).xyz);
R1f.xyz = (texture(textureUnitPS6, R1f.xy).xyz);
R0f.xyz = (texture(textureUnitPS1, R0f.xy).xyz);
// 0
PV0f.x = fract(R2f.x);
R126f.y = (R5f.x * intBitsToFloat(0x40008102) + intBitsToFloat(0xbf810204));
PV0f.y = R126f.y;
R127f.z = mul_nonIEEE(R3f.y, R4f.z);
PV0f.w = fract(R2f.y);
R126f.z = mul_nonIEEE(R3f.z, R4f.x);
PS0f = R126f.z;
// 1
PV1f.x = mul_nonIEEE(R3f.x, R4f.y);
PV1f.y = PV0f.w + -(0.5);
PV1f.z = PV0f.x + -(0.5);
R127f.w = (R5f.y * intBitsToFloat(0x40008102) + intBitsToFloat(0xbf810204));
PV1f.w = R127f.w;
PS1f = mul_nonIEEE(PV0f.y, PV0f.y);
// 2
R123f.x = (mul_nonIEEE(-(PV1f.z),PV1f.z) + 1.0);
R123f.x = clamp(R123f.x, 0.0, 1.0);
PV0f.x = R123f.x;
R127f.y = (mul_nonIEEE(-(R4f.y),R3f.z) + R127f.z);
R127f.z = (mul_nonIEEE(-(R4f.x),R3f.y) + PV1f.x);
R123f.w = (mul_nonIEEE(-(PV1f.y),PV1f.y) + 1.0);
R123f.w = clamp(R123f.w, 0.0, 1.0);
PV0f.w = R123f.w;
R122f.x = (mul_nonIEEE(PV1f.w,PV1f.w) + PS1f);
R122f.x = clamp(R122f.x, 0.0, 1.0);
PS0f = R122f.x;
// 3
PV1f.x = -(PS0f) + 1.0;
PV1f.y = mul_nonIEEE(R4f.w, R127f.w);
PV1f.z = mul_nonIEEE(PV0f.x, PV0f.w);
R123f.w = (mul_nonIEEE(-(R4f.z),R3f.x) + R126f.z);
PV1f.w = R123f.w;
R125f.z = mul_nonIEEE(R6f.x, R1f.x);
PS1f = R125f.z;
// 4
PV0f.x = mul_nonIEEE(R127f.y, PV1f.y);
PV0f.y = mul_nonIEEE(PV1f.z, PV1f.z);
PV0f.z = mul_nonIEEE(R127f.z, PV1f.y);
PV0f.w = mul_nonIEEE(PV1f.w, PV1f.y);
R127f.z = sqrt(PV1f.x);
PS0f = R127f.z;
// 5
R123f.x = (mul_nonIEEE(R4f.y,R126f.y) + PV0f.w);
PV1f.x = R123f.x;
R123f.y = (mul_nonIEEE(R4f.x,R126f.y) + PV0f.x);
PV1f.y = R123f.y;
R126f.z = mul_nonIEEE(R1f.w, PV0f.y);
R123f.w = (mul_nonIEEE(R4f.z,R126f.y) + PV0f.z);
PV1f.w = R123f.w;
R126f.y = mul_nonIEEE(R6f.z, R1f.z);
PS1f = R126f.y;
// 6
R124f.x = (mul_nonIEEE(R3f.x,R127f.z) + PV1f.y);
R124f.y = (mul_nonIEEE(R3f.y,R127f.z) + PV1f.x);
R1f.z = (mul_nonIEEE(R3f.z,R127f.z) + PV1f.w);
R127f.w = mul_nonIEEE(R6f.y, R1f.y);

#if (gsswDefault == 1) // Default line in section 6

R126f.w = mul_nonIEEE(intBitsToFloat(uf_remappedPS[0].x), R7f.x);

#elif (gsswDefault == 0) // Modified line in section 6

R126f.w = mul_nonIEEE(Color.r, R7f.x);

#endif

PS0f = R126f.w;

#if (gsswDefault == 1) // Default section 7

// 7
R127f.x = mul_nonIEEE(intBitsToFloat(uf_remappedPS[0].x), PS0f);
R127f.y = mul_nonIEEE(intBitsToFloat(uf_remappedPS[0].y), R7f.y);
PV1f.z = R126f.z * intBitsToFloat(0x427f0000);
R125f.w = mul_nonIEEE(intBitsToFloat(uf_remappedPS[0].z), R7f.z);
R124f.z = intBitsToFloat(0x3d008081);
PS1f = R124f.z;

#elif (gsswDefault == 0) // Modified section 7

// 7
R127f.x = mul_nonIEEE(Color.r, PS0f);
R127f.y = mul_nonIEEE(Color.g, R7f.y);
PV1f.z = R126f.z * intBitsToFloat(0x427f0000);
R125f.w = mul_nonIEEE(Color.b, R7f.z);
R124f.z = intBitsToFloat(0x3d008081);
PS1f = R124f.z;

#endif

// 8
R123f.x = (mul_nonIEEE(-(R5f.z),intBitsToFloat(uf_remappedPS[1].z)) + -(intBitsToFloat(uf_remappedPS[1].y)));
R123f.x = clamp(R123f.x, 0.0, 1.0);
PV0f.x = R123f.x;

#if (gsswDefault == 1) // Default part of section 8

R125f.y = mul_nonIEEE(R125f.z, intBitsToFloat(uf_remappedPS[1].x));
PV0f.y = R125f.y;
R127f.z = mul_nonIEEE(R127f.w, intBitsToFloat(uf_remappedPS[1].x));
PV0f.z = R127f.z;
R127f.w = mul_nonIEEE(R126f.y, intBitsToFloat(uf_remappedPS[1].x));

#elif (gsswDefault == 0) // Modified part of section 8

R125f.y = mul_nonIEEE(R125f.z, intBitsToFloat(uf_remappedPS[1].x) * Factor);
PV0f.y = R125f.y;
R127f.z = mul_nonIEEE(R127f.w, intBitsToFloat(uf_remappedPS[1].x) * Factor);
PV0f.z = R127f.z;
R127f.w = mul_nonIEEE(R126f.y, intBitsToFloat(uf_remappedPS[1].x) * Factor);

#endif

PV0f.w = R127f.w;
R126f.y = floor(PV1f.z);
R126f.y *= 4.0;
PS0f = R126f.y;
// 9
backupReg0f = R126f.w;
R126f.x = mul_nonIEEE(R127f.y, PV0f.z);

#if (gsswDefault == 1) // Default line in section 9

PV1f.y = mul_nonIEEE(intBitsToFloat(uf_remappedPS[0].y), R127f.y);

#elif (gsswDefault == 0) // Modified line in section 9

PV1f.y = mul_nonIEEE(Color.g, R127f.y);

#endif

R125f.z = mul_nonIEEE(intBitsToFloat(uf_remappedPS[1].w), PV0f.x);
PV1f.z = R125f.z;
R126f.w = mul_nonIEEE(backupReg0f, PV0f.y);
R125f.x = mul_nonIEEE(R125f.w, PV0f.w);
PS1f = R125f.x;
// 10
backupReg0f = R126f.y;

#if (gsswDefault == 1) // Default line in section 10

PV0f.x = mul_nonIEEE(intBitsToFloat(uf_remappedPS[0].z), R125f.w);

#elif (gsswDefault == 0) // Modified line in section 10

PV0f.x = mul_nonIEEE(Color.b, R125f.w);

#endif

R126f.y = mul_nonIEEE(PV1f.z, R127f.x);
R126f.z = mul_nonIEEE(PV1f.z, PV1f.y);
R125f.w = intBitsToFloat(uf_remappedPS[2].z);
R127f.x = backupReg0f + 2.0;
PS0f = R127f.x;
// 11
backupReg0f = R125f.z;
tempf.x = dot(vec4(R124f.x,R124f.y,R1f.z,-0.0),vec4(R124f.x,R124f.y,R1f.z,0.0));
PV1f.x = tempf.x;
PV1f.y = tempf.x;
PV1f.z = tempf.x;
PV1f.w = tempf.x;
R125f.z = tempf.x;
PS1f = mul_nonIEEE(backupReg0f, PV0f.x);
// 12
R5f.x = (mul_nonIEEE(R126f.y,R125f.y) + R126f.w);
R5f.y = (mul_nonIEEE(R126f.z,R127f.z) + R126f.x);
R5f.z = (mul_nonIEEE(PS1f,R127f.w) + R125f.x);
R1f.w = 1.0;
R1f.x = R124f.z;
PS0f = R1f.x;
// 13
R1f.y = R125f.w;
R5f.w = 1.0;
R7f.w = R127f.x * intBitsToFloat(0x3b808081);
PS1f = R7f.w;
// 14
R0f.w = intBitsToFloat(0x3ec2c2c4);
tempResultf = 1.0 / sqrt(R125f.z);
PS0f = tempResultf;
PS0f /= 2.0;
// 15
R7f.x = (mul_nonIEEE(R124f.x,PS0f) + 0.5);
R7f.y = (mul_nonIEEE(R124f.y,PS0f) + 0.5);
R7f.z = (mul_nonIEEE(R1f.z,PS0f) + 0.5);
// 16
backupReg0f = R5f.x;
backupReg1f = R5f.y;
backupReg2f = R5f.z;
backupReg3f = R5f.w;
R5f.xyz = vec3(backupReg0f,backupReg1f,backupReg2f);
R5f.w = backupReg3f;
// 17
R4f.xyz = vec3(R7f.x,R7f.y,R7f.z);
R4f.w = R7f.w;
// 18
R3f.xyz = vec3(R0f.x,R0f.y,R0f.z);
R3f.w = R0f.w;
// 19
R2f.xyz = vec3(R1f.x,R1f.y,R1f.z);
R2f.w = R1f.w;
// export
passPixelColor0 = vec4(R2f.x, R2f.y, R2f.z, R2f.w);
passPixelColor1 = vec4(R3f.x, R3f.y, R3f.z, R3f.w);
passPixelColor3 = vec4(R4f.x, R4f.y, R4f.z, R4f.w);
passPixelColor5 = vec4(R5f.x, R5f.y, R5f.z, R5f.w);
}
